# Run Auto Calibration

You can use the auto calibration commands if you want the AlignSight application to provide the calibration positions. When you use auto calibration, the only calibration position you need to train or configure is the calibration starting position.

To perform auto calibration, run the auto calibration commands in the following sequence:

Note:

- For more information about auto calibration commands, see Automatic Calibration.
- The pose position (X, Y, A) provided to the ACB command to initialize the auto calibration should have the calibration feature presented approximately in the center of the field of view.