# Alignment Commands

Use the alignment commands to train the golden pose position of the part.

The training steps include the following:

1. Train the feature using the AlignSight software.
2. Run the TA command to register the golden position of the part.
3. Run the XA command to get the coordinates that the moving station must move to bring that part from an arbitrary run-time position back to the golden position.