# Automatic Calibration

Use automatic calibration to determine the position of the camera within the coordinate space of the motion system, without having to train the positions of the motion system. Calibration positions are provided by AlignSight.

Automatic calibration is a two-step process:

1. Move the motion system to a position where the trained feature is in the center of the field of view of the camera to be calibrated.
2. Run the ACB command.
3. Use the AC command to execute the automatic calibration.

Note: Automatic calibration does not support simultaneous calibration of multiple cameras.