# Two Camera Systems

### 1 Feature Per Camera Configuration

This configuration will be loaded by default when a new Recipe is created for a two-camera sensor.

PartID | Camera | Camera Feature | Exposure
--- | --- | --- | ---
1 | 1 | 1 | 1, -
2 | 2 | 1 | -, 1
3 | 1 + 2 | 1 + 1 | 1, 1

StepID | Locates | Exposure | Calibration
--- | --- | --- | ---
1 | Part 1 | 1, - | 1
2 | Part 2 | -, 1 | 1
3 | Part 3, PF 1 + 2 | 1, 1 | 1
4 | Part 3, PF 1 | 1, - | 1
5 | Part 3, PF 2 | -, 1 | 1

### 2 Features Per Camera Configuration

This configuration supports a total of four features (two per camera).

PartID | Camera | Camera Feature | Exposure
--- | --- | --- | ---
1 | 1 | 1 | 1, -
2 | 1 | 2 | 2, -
3 | 1 | 1 + 2 | 1, -
4 | 2 | 1 | -, 1
5 | 2 | 2 | -, 2
6 | 2 | 1 + 2 | -, 1

StepID | Locates | Exposure | Calibration
--- | --- | --- | ---
1 | Part 1 | 1, - | 1
2 | Part 2 | 2, - | 1
3 | Part 3, F1 + 2 | 1, - | 1
4 | Part 4 | -, 1 | 1
5 | Part 5 | -, 2 | 1
6 | Part 6, F1 + 2 | -, 1 | 1
7 | Part 3, F1 | 1, - | 1
8 | Part 3, F2 | 2, - | 1
9 | Part 6, F1 | -, 1 | 1
10 | Part 6, F2 | -, 2 | 1