### Set Product ID

PID

Sets the product ID which is used as a prefix for the image filename in image logging.

<ProductID>_<YYYYMMDD>_<hhmmss>_<command>

#### TCP/IP:

Command String:

PID,<ProductID>

Field | Arguments
--- | ---
PID | The command
<ProductID> | Product ID used as prefix during image logging. String or numeric value

Result String:

PID, <Status>

Field | Arguments
--- | ---
PID | The command
<Status> | The result status 1: Success <=0: Fail

#### SLMP:

Send command (Input Block)

Offset | Value | Description
--- | --- | ---
VIB_Offset + 2 | 5050 | Command: PID command ID
VIB_Offset + 3 | <ProductID> | Product ID used as prefix during image logging. Only numeric value

Receive Result (Output Block)

Offset | Value | Description
--- | --- | ---
VOB_Offset + 5 | 5050 | Command: PID command ID
VOB_Offset + 6 | <Status> | Argument0: The result Status: 1: Success <=0: Fail