### SLMP

The above native commands can be executed in SLMP scanner mode by sending the command strings through the String Cmd Block.

Result strings are returned in the String Result Block.

See InSight SLMP documentation for further details.

Note: Only the Native commands to load a recipe and to set the Startup job are supported by AlignSight. These commands must only be sent to the Master camera.
Executing other Native commands, in particular when the Setup HMI is active, may have unpredictable results.