### Get Version

GV

Returns the current version of the loaded recipe.

#### TCP/IP:

Command String:

GV,<cam>

Field | Arguments
--- | ---
GV | The command
<cam> | The camera(s) to be read 0: All available cameras 1: Camera 1 only 2: Camera 2 only

Result String:

GV,<Status>,<Major>,<Minor>,<SubMinor>

Field | Arguments
--- | ---
GV | The command
<Status> | The result status 1: Success <=0: Fail
<Major> | The Major Version
<Minor> | The Minor Version
<SubMinor> | The Sub Minor Version

#### SLMP:

Send command (Input Block)

Offset | Value | Description
--- | --- | ---
VIB_Offset + 2 | 1011 | Command: GV command ID
VIB_Offset + 3 | <cam> | Argument0: The camera(s) to be read

Receive Result (Output Block)

Offset | Value | Description
--- | --- | ---
VOB_Offset + 5 | 1011 | Command: GV command ID
VOB_Offset + 6 | <Status> | The result Status: 1: Success <=0: Fail
VOB_Offset + 7 | <Major> | The Major Version
VOB_Offset + 9 | <Minor> | The Minor Version
VOB_Offset + 11 | <SubMinor> | The Sub Minor Version