### TCP

A Recipe change using TCP command is not supported by In-Sight. Therefore, a set of native commands must be sent via a telnet connection (Port 23) to the Master camera:

- Close TCP connection

- Open a Telnet connection to the Master In-Sight (user = “admin”, Password = “” ).

- Execute native command: “SO0” (Set Offline)

- Execute native command: “LF<RecipeName>” (Load File)

- Execute native command: “SO1” (Set Online)

- Close Telnet connection

- Open TCP connection

  Note: The Recipe filename consists of the Recipe ID (3 digits) and the Recipe name, e.g.