# Run Mode (Home)

You can monitor a running AlignSight.

Number | Element | Description
--- | --- | ---
1 | Home Button | Open the Home screen.
2 | Setup Navigation Pane | Connect an AlignSight.
3 | Exit Button | Close the AlignSight software.
4 | Information Bar | Displays the sensor and recipe currently in use.
5 | Image Viewer Controls | Zooms in, zooms out, or fits image to the display.
6 | Live Mode Toggle | Displays a live video image to use when you adjust the cameras lens and the field of view.
7 | Rotate Image Controls | Rotates the image 90 degrees clockwise or counterclockwise.
8 | Save Image Button | Saves images.
9 | Language Selection | Selects the language to use in the AlignSight user interface.
10 | Access Control | You can log on to your AlignSight as the Admin or Operator. After you log off, you can still use the AlignSight software as the Monitor.
11 | Help | Opens the AlignSight documentation.
12 | Camera Image View | Displays the sensor's view.
13 | Message Window | Displays the sensor's log.
14 | Calibration Quality Indicators | Displays the calibration quality of the system's camera(s).
15 | Status Bar | Displays the user, version, and date, and time information.
16 | Checkerboard Calibration | Configure checkerboard calibration to eliminate lens distortion errors.
17 | Recipe | Create, edit and delete recipes.
18 | Control Panel | Open the Control Panel to connect to a robot controller and control robot movements

Mouse operations on image:

Mouse wheel | Up/down move of enlarged image
Shift + Ctrl + left-click drag | Move enlarged image
Ctrl + left-click | Zoom in at click position as center
Ctrl + left-click drag | Zoom into area selected with clicked point as center
Shift + Mouse wheel | Zoom in/out against FOV center

Note:

When a system uses two cameras, the following controls apply to only the selected camera that displays in a white frame:

- Image View controls
- Live Mode toggle
- Rotate Image controls
- Save Image button