# Setup Mode (Sensor)

You can configure, modify and delete sensors.

Number | Element | Description
--- | --- | ---
1 | Context Help Pane | Displays the instructions.
2 | Information Bar | Selects a sensor (if multiple sensors exist) and adds or deletes a sensor.
3 | Setup Windows | Configures, modifies, and deletes sensors.
4 | Backup Data Button | Backs up sensor's recipe, calibration, and configuration data.
5 | Restore Data Button | Restores the recipe, calibration, and configuration data to a sensor.
6 | Advanced Settings Button | Opens the Advanced Settings window.
7 | Status Bar | Displays the user, version, and date, and time information.
8 | Communications | TCP/IP settings including the message length header. If it is checked, the sensor begins the response with a 3-digit header indicating the response length excluding the CR/LF.
9 | Reset Sensor | Reset the Sensor and performs a physical power cycling on the camera.