# Handedness of Coordinate Spaces

Independent handedness is assumed among Home2D, Camera2D, and Plate2D. The Home2D handedness is determined by the directions of the motion stage's axes. The Plate2D handedness comes with the calibration plate artwork design. The Camera2D handedness is determined by the number of mirrors in the optical path. These are naturally independent of each other, and are treated as such.