# Camera Shuttling or Part Shuttling

In some applications, cameras are shuttled or the parts are shuttled to detect the pose of parts.

## Camera Shuttling

Camera acquires image from one side of the part first, then shuttles to the other side of the part and acquires again. The vision system will combine information from the different images for processing.

## Part Shuttling

Cameras acquire images on one side of the part, then the part itself moved by platform to the other side under the cameras, then cameras take another set of images. The vision system will combine all information from different images for processing.

The work flow for vision is as below:

Note that this camera shuttling could be more than 2 positions. AlignPlus supports multiple camera shuttling positions.