# Event Responses

The event can also be given a response. It is configured by defining the output bank and line number on which it will be sent, the signal transition, pulse width, and optionally, a delay that specifies when the output will be fired, after a specific amount of time (0 to 10000 ms).

Note: The DS1000OutputBank is only available when connected to a Vision Controller Communication Card.