# SLMP PLC Remote Station Configuration

The Remote Station is used to configure the connection information required to establish a connection between the vision system and the Mitsubishi PLC/MC.

Settings | Description
--- | ---
Station ID | Specifies the station ID (ID of C24 on a multi-drop serial connection); also used as the PCID field for 1E/3E frames.
Network ID | Specifies the SLMP network number (0 to 239; default = 0) that will be used to communicate (0 = the local network).
Destination Station | Specifies the Remote Station Destination Station ID, which is the ID of the second hop station (also the PCID for 1C frames).
Destination Module | Specifies the identifier of the device module that the vision system will be connected to.
LocalStation_0x3FF | 0x3FF
ControlSystemCPU_0x3D0 | 0x3D0
StandbySystemCPU_0x3D1 | 0x3D1
SystemACPU_0x3D2 | 0x3D2
SystemBCPU_0x3D3 | 0x3D3
CPU 1_0x3E0 | 0x3E0
CPU 2_0x3E1 | 0x3E1
CPU 3_0x3E2 | 0x3E2
CPU 4_0x3E3 | 0x3E3