# SLMP Control Bit Signal Table

The SLMP Control Bit signal table/block organizes the single bit NDM signals sent FROM the PLC to the vision system. The Control Bit block is 80 bits long.

Byte | Bit 7 | Bit 6 | Bit 5 | Bit 4 | Bit 3 | Bit 2 | Bit 1 | Bit 0
--- | --- | --- | --- | --- | --- | --- | --- | ---
0 | Set Offline | Clear Error | Reserved | Initiate Job Load | Reserved | Reserved | Buffer Results Enable | Trigger Enable
1 | Reserved
2-5 | Soft Event 0-31
6 | Reserved | Reserved | Reserved | Reserved | Set User Data 0 | Clear Exposure Complete 0 | Inspection Results Acknowledge 0 | Trigger Camera 0
7 | Reserved | Reserved | Reserved | Reserved | Set User Data 1 | Clear Exposure Complete 1 | Inspection Results Acknowledge 1 | Trigger Camera 1
8 | Reserved | Reserved | Reserved | Reserved | Set User Data 2 | Clear Exposure Complete 2 | Inspection Results Acknowledge 2 | Trigger Camera 2
9 | Reserved | Reserved | Reserved | Reserved | Set User Data 3 | Clear Exposure Complete 3 | Inspection Results Acknowledge 3 | Trigger Camera 3