# Import Rung

Currently, Designer does not have an Add-On Profile (AOP), so an import rung has been created to copy the raw data from the Cognex Communication Card or Vision Controller into the User Defined Data Type (UDT), with tags, to improve access. The import rung is located at: C:\Program Files\Cognex\VisionPro\ffp\eds\VisionController_Copy_Run.L5X

The imported rung should be placed at the beginning of the main routine.

Note: In this example, a Generic Ethernet Module is being used, so the import rung is necessary.

The UDTs that are imported will have a tag name associated with all the data points that come in and out of the Cognex Communication Card/Vision Controller.