# Precision I/O Overview

In a typical production environment, the vision application on the host PC must acknowledge and process incoming I/O signals before responding with appropriate outgoing signals:

By defining a precision I/O event system, the vision application can load a predefined set of precision I/O events onto the Cognex Communication Card and allow the processor on the card to read input lines and generate the appropriate response by setting desired output lines: