# SLMP Status Bit Signal Table

The SLMP Status Bit signal table/block organizes the single bit NDM signals sent FROM the vision system to the PLC. The Status Bit block is 112 bits long.

Byte | Bit 7 | Bit 6 | Bit 5 | Bit 4 | Bit 3 | Bit 2 | Bit 1 | Bit 0
--- | --- | --- | --- | --- | --- | --- | --- | ---
0 | Online | Offline Reason | Reserved | Reserved | System Busy | System Ready
1 | General Fault | Reserved | Job Load Completed | Reserved | Reserved | Reserved | Reserved | Reserved
2-5 | Soft Event Acknowledge 0-31
6 | Results Buffer Overrun 0 | Inspection Passed 0 | Results Valid 0 | Inspection Completed 0 | Exposure Complete 0 | Acq Error 0 | Trigger Acknowledge Camera 0 | Trigger Ready Camera 0
7 | Reserved | Reserved | Reserved | Reserved | Reserved | Reserved | Reserved | Set User Data Ack 0
8 | Results Buffer Overrun 1 | Inspection Passed 1 | Results Valid 1 | Inspection Completed 1 | Exposure Complete 1 | Acq Error 1 | Trigger Acknowledge Camera 1 | Trigger Ready Camera 1
9 | Reserved | Reserved | Reserved | Reserved | Reserved | Reserved | Reserved | Set User Data Acknowledge 1
10 | Results Buffer Overrun 2 | Inspection Passed 2 | Results Valid 2 | Inspection Completed 2 | Exposure Complete 2 | Acq Error 2 | Trigger Acknowledge Camera 2 | Trigger Ready Camera 2
11 | Reserved | Reserved | Reserved | Reserved | Reserved | Reserved | Reserved | Set User Data Acknowledge 2
12 | Results Buffer Overrun 3 | Inspection Passed 3 | Results Valid 3 | Inspection Completed 3 | Exposure Complete 3 | Acq Error 3 | Trigger Acknowledge Camera 3 | Trigger Ready Camera 3
13 | Reserved | Reserved | Reserved | Reserved | Reserved | Reserved | Reserved | Set User Data Acknowledge 3