# PCM.METRIC-PARM-THRESHOLD

Set the raw value threshold for the selected quality standard, metric and grade (e.g. AIM-DPM → UEC → Threshold B = 50). Not all metrics are available for each standard: AIM-DPM (0, 1, 3, 4, 6, 8), ISO-IEC 15415 (0, 1, 3, 4, 6), ANSI-ISO-IEC 15416 (1, 4, 8, 9, 23, 25), 1D readability (0, 2, 8, 9, 11), DotCode (0, 1, 2, 3, 6, 8)

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
type |  | [0-5] | 0: AIM-DPM 1: ISO-IEC 15415 2: ANSI-ISO-IEC 15416 3: SemiT10 4: 1D readability 5: DotCode Readybility
type |  | [0-25] | 0: Symbol Contrast 1: Axial Non Uniformity 2: Print Growth 3: UEC 4: Modulation 5: Fixed Pattern Damage 6: Grid Non Uniformity 7: Extreme Reflectance 8: Reflect Min 9: Edge Contrast Min 10: Single Scan Int 11: Multi Scan Int 12: Signal To Noise Ratio 13: Horizontal Mark Growth 14: Vertical Mark Growth 15: Data Matrix Cell Width 16: Data Matrix Cell Height 17: Horizontal Mark Misplacement 18: Vertical Mark Misplacement 19: Cell Defects 20: Finder Pattern Defects 21: Overall Grade 22: Edge Determination 23: Defects 24: Reference Decode 25: Decodability
grade |  | [1-4] | 1: D 2: C 3: B 4: A Threshold raw value
value |  | [0-1000] |

## Platforms

Ethernet readers.

## Notes

Version: 5.7.0