View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# How can I reset the USB connection to the base station?

If you have difficulty establishing or maintaining a USB connection between a base station and your PC, follow these steps to reset the USB connection:

1. Disconnect both the USB cable and the power cable from the base station.

2. Reconnect both the USB cable and the power cable to the base station.

3. Place the reader in the base station.

4. Remove the reader from the base station and scan the USB-COM/RS_232 configuration code.

Note: default,DM8050,DM8070,DM8600,DM8700,DM8700Base,DM8000Base