# Connecting a DataMan 8072 ER Through Ethernet

1. Connect the Ethernet slide-in (DMCM-ENETM-00) to your DataMan 8072 ER.

2. With a 2.5 mm Allen wrench, tighten the screws so that the slide-in is firmly locked.

3. Insert the plug. Slide the cable lock up to the reader, and twist the cable lock in place.

Use the DM8000-ECABLE-05 (5 meters) or the DM8000-ECABLE-30 (30 meters). You also need a Power Over Ethernet Adapter (CPS-AC-POE1A-xx).

Note: Disconnect the DataMan 8072 ER reader from power before inserting/removing communication modules.