# DataMan 8072 ER Specifications

Specification | DataMan 8072 ER Reader
--- | ---
Weight | 254g Wireless: 530 g (18.70 oz) (battery included)
Operating Temperature | 0 ºC — 40 ºC (32 ºF — 104 ºF)
Storage Temperature | -10 ºC — 60 ºC (14 ºF — 140 ºF)
Maximum Humidity | < 95% (non-condensing)
Environmental | IP65
Symbologies | 1-D barcodes: Codabar, Code 39, Code 128, and Code 93, Interleaved 2 of 5, Pharma, GS1 DataBar, Postal, UPC/EAN/JAN, DataBar 2-D barcodes: Data MatrixTM; QR Code and microQR Code, RSS/CS, PDF 417, MicroPDF 417, MaxiCode, Aztec Code
Power Supply Requirements | USB: external 5.0 W maximum LPS or NEC class 2 power supply: +5 V - +6 V DC RS232 external 5.0 W max LPS or NEC class 2 power supply
Inrush current peak | 5A maximum Duration: approx. 30 μs Electrical charge: 60 μAs at 6 V Maximum capacity: 10 µF Maximum inrush: 50 µC
Battery life for wireless reader (typical use case) | ca. 4100 triggers can be operated within a 13 hour working shift The expected life time of the battery is 5 years.
Ethernet | 10/100 Base-T FULL/HALF DUPLEX, IEEE 802.3
Bluetooth | Bluetooth™ 2.1, 2.4 GHz
Protection |