# Physical Layout of the Base Station

DMA-IBASE-BT-02

1 | Base station status indicators
2 | PAIR sticker - Reading the code pairs the base station with the device
3 | Connection point to the reader: pairing reader and base station non-wireless communication charging
4 | RS-232
5 | USB
6 | Power plug (24 V, max. 15 W)
7 | Alternative power supply connector (24 V, max. 15 W, polarity marked on the plastic part near the connector). Recommended wire diameter is 14- 18 AWG
8 | Ethernet

DMA-IBASE-BT-02

1 | Base station status indicators
2 | PAIR sticker - Reading the code pairs the base station with the device
3 | Connection point to the reader: pairing reader and base station non-wireless communication charging
4 | RS-232
5 | USB
6 | Power plug (24 V, max. 15 W)
7 | Alternative power supply connector (24 V, max. 15 W, polarity marked on the plastic part near the connector). Recommended wire diameter is 14- 18 AWG
8 | Ethernet

Base Station status indicators:

- Power: RED = base powered / BLINK = wrong reader in base
- Communication: BLUE = Wireless link / BLINK = Wireless communication
- Cradle connections: GREEN = reader properly inserted / BLINK = cradle USB interface communication

Note:

- DMA-IBASE-BT-02 supports Ethernet