# Camera Overview

Command | Supported Platforms
--- | ---
CAMERA.AUTO-REGULATION | DM50, DM60, DM70, DM80, DM150, DM260, DM280, DM503, DM8600, and DM300, DM360, DM370, DM470
CAMERA.BURST-LENGTH | Fixed mount readers.
CAMERA.EXPOSURE | DM50, DM60, DM70, DM80, DM150, DM260, DM280, DM360, DM370, DM470, DM503
CAMERA.EXPOSURE-LIMIT-US | Fixed Mount readers.
CAMERA.EXPOSURE-US | DM50, DM60, DM70, DM150, DM260
CAMERA.EXPOSURE-US | DM80, DM280, DM370, DM470, DM580, DM8700
CAMERA.EXPOSURE-US | DM300, DM360, DM8600
CAMERA.EXPOSURE-US | DM503
CAMERA.FOV | ALL
CAMERA.FOV-ENABLED | ALL
CAMERA.FULL-BLACK-LEVEL-CORRECTION | DM300, DM360
CAMERA.GAIN | DM50, DM60, DM70, DM80, DM280, DM300, DM360, DM370, DM470, DM503
CAMERA.GAIN-LIMIT | Fixed-mount readers
CAMERA.HDR-MODE | DM80, DM280, DM370, DM470
CAMERA.HDR-MODE | DM370.
CAMERA.INTERVAL-US | DM50, DM60, DM70, DM80, DM280, DM300, DM360, DM370, DM470, DM503
CAMERA.MAX-EXPOSURE-US | DM70, DM80, DM150, DM260, DM280, DM300, DM360, DM370, DM470, DM503
CAMERA.MAX-EXPOSURE-US | DM50, DM60, DM70.
CAMERA.MIRROR-HORIZONTAL | DM80, DM280, DM300, DM360, DM370, DM470, DM503
CAMERA.MIRROR-VERTICAL | DM70, DM80, DM260, DM280, DM300, DM360, DM370, DM470, DM503
CAMERA.ROI |
CAMERA.TARGET-BRIGHTNESS | All, except MX.
CAMERA.XPAND-ROI | DM70, DM150, DM260, DM300, DM360, DM370, DM470, DM503.
CAMERA.XPAND-ROI-TYPE | DM70, DM150, DM260, DM300, DM360, DM370, DM470, DM503.
DEVICE.LENS-SERIAL | ALL
FOCUS.AUTOFOCUS.MID-RANGE | MX-1502 ER and XR
FOCUS.DISTANCE | DM300, DM360, DM370, DM470
FOCUS.EXTENDED-RANGE | Fixed-mount readers with Liquid Lens
FOCUS.FEEDBACK | DM80, DM280, DM300, DM360, DM370, DM470, DM503
FOCUS.POWER | Fixed-mount readers with Liquid Lens
FOCUS.PRECISION | Fixed mount readers with a liquid lens.
FOCUS.PROGRESS | Fixed mount readers with a liquid lens.
FOCUS.SWEEP-POWER | Readers with Liquid Lens.
FOCUS.SWEEP-RANGE | DM70, DM260, DM300, DM360, DM370, DM470, DM8000
FOCUS.SWEEP-STEPS | DM70, DM80, DM260, DM280, DM300, DM360, DM370, DM470, DM8000
HEIGHT-SENSOR.CURRENT-MEASUREMENT | DM370, DM470.
IMAGE.FORMAT | ALL
IMAGE.QUALITY | ALL
IMAGE.SEND-SLOT |
IMAGE.SEND-TYPE |
IMAGE.SIZE | ALL
LIGHT.AIMER | ALL except for DM503 and DM8050
LIGHT.AIMER | DM8050
LIGHT.AIMER | DM370, DM470 readers.
LIGHT.AIMER-TIMEOUT | MX-1000 and DM8000.
LIGHT.BANKS | DM8700 DX
LIGHT.COLOR-CHANNELS | DM282 with HPIT.
LIGHT.DARKFIELD-INTENSITY | DM8600
LIGHT.DIFFUSE-INTENSITY | DM8600
LIGHT.DIRECT | DM80, DM280, DM300, DM360, DM370, DM470
LIGHT.DIRECT | DM70, DM150 and DM260 readers
LIGHT.DIRECT | DM370, DM470.
LIGHT.DIRECT-INTENSITY | DM50, DM60, DM300, DM360, DM370, DM470, DM503
LIGHT.DIRECT-INTENSITY | DM8050
LIGHT.EXTERNAL-ENABLE | Fixed mount readers.
LIGHT.EXTERNAL-INTENSITY | Fixed mount readers.
LIGHT.EXTERNAL-POLARITY | Fixed mount readers except for DM70, DM150, DM260.
LIGHT.EXTERNAL-PRECHARGE-TIME | Fixed mount readers.
LIGHT.HIGH-FREQUENCY | DM50, DM60, DM70, DM80, DM280, DM300, DM360, DM370, DM470, DM503
LIGHT.HIGH-FREQUENCY-ALWAYS | DM50, DM60, DM70, DM80, DM280, DM300, DM360, DM370, DM470, DM503
LIGHT.INTERNAL-ENABLE | DM50, DM60, DM70, DM8050, MX-1000, MX-1502, Mobile.
LIGHT.LOW-ANGLE | DM262
LIGHT.ON-AXIS | DM262
LIGHT.POLARIZED | DM70, DM80, DM150, DM260, DM280
LIVEIMG.MODE | ALL
LIVEIMG.SEND |
MASTER-SLAVE.RX-HEIGHT-SENSOR | DM60, DM80-PoE, DM280, DM300, DM360, DM370, DM470.
MIRROR.CURRENT-INDEX | DM370, DM470 equipped with High Speed Steerable Mirror
MIRROR.ENABLE-FOCUS-CORRECTION | DM370, DM470 equipped with High Speed Steerable Mirror
MIRROR.PATH | DM370, DM470 equipped with High Speed Steerable Mirror
MIRROR.PATH-ENABLE | DM370, DM470 equipped with High Speed Steerable Mirror
MONITOR-MODE.AUTOEXPOSURE | ALL
MONITOR-MODE.DECODE-ENABLE | ALL
MONITOR-MODE.ENABLE | ALL
SETUP.ENABLE | DM50, DM60, DM70, DM80, DM150, DM260, DM280, DM300, DM360, DM370, DM470, DM503, DM8600, MX-1000
SETUP.ENABLE-SINGLE | DM370, DM470
SETUP.NAME | DM50, DM60, DM70, DM80, DM150, DM260, DM280, DM300, DM360, DM370, DM470, DM503, DM8600, MX-1000
SETUP.PROG-TARGET | DM80, DM280, DM8600
SETUP.PROG-TARGET | DM50, DM60, DM70, DM150, DM260, DM300, DM360, DM370, DM470, DM503, MX-1000, and MX-1502
SETUP.PROG-TARGET | DM8700
SETUP.START-WITH-LAST-READ | DM8600, DM70, DM80, DM150, DM260, DM280, DM300, DM360, DM370, DM470, DM503, MX-1000, MX-1502
SETUP.START-WITH-SETUP | DM8600, DM70, DM80, DM150, DM260, DM280, DM300, DM360, DM370, DM470, DM503, MX-1000, MX-1502
TRIGGER.DELAY-DISTANCE | DM80, DM280, DM300, DM360, DM370, DM470, DM503
TRIGGER.DELAY-TIME | DM50, DM60, DM70, DM300, DM360, DM370, DM470, DM503
TRIGGER.DELAY-TYPE | DM50, DM60, DM70, DM80, DM280
TRIGGER.DELAY-TYPE | DM80, DM280, DM300, DM360, DM370, DM470, DM503
TRIGGER.END-DELAY-DISTANCE | DM80, DM280, DM300, DM360, DM370, DM470, DM503
TRIGGER.END-DELAY-TIME | DM50, DM60, DM70, DM80, DM280, DM300, DM360, DM370, DM470, DM503
TRIGGER.TYPE | DM80, DM280. DM8000 supports only Presentation and Manual trigger types. MX-1000, MX-1502 and Mobile support only Manual and Continuous trigger types.
TUNE.ADJUST-FOCUS | DM70, DM150, DM260, DM300, DM360, DM370, DM470 with liquid lens.
TUNE.EXCLUDE-AMBIENT-RESULTS | Fixed mount readers.
TUNE.TRAIN-CODE | DM80, DM280, DM300, DM360, DM370, DM470, DM70, DM260, and DM150.
TUNE.TUNE-LIGHT-BANKS | DM300, DM360, DM370, DM470, DM260, DM70 and DM150.
TUNE.TUNE-LIGHT-COMBINATIONS | DM300, DM360, DM370, DM470, DM260, DM70 and DM150.