View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is the Automatic Reader Configuration Backup?

Automatic Backup works with devices connected through Ethernet. When enabled, this function does a device configuration backup to an external storage (an FTP server) every time the configuration is saved to flash. A Cognex Explorer service can receive the backup data. Restore can be done manually by either Setup Tool, DMCC commands or Cognex Explorer.

Configure the reader with the IP address and port number necessary to specify where you want to save the configuration. You can also set a username and password combination.

Note: default,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM080, DM280, DM470,DM580, DM503,DM8050,DM8070,DM8600,DM8700,DM8700Base,DM8000Base