View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# Why am I not able to try my trigger command or echoing commands in a terminal program?

Custom commands are provided to be used by a PLC or similar device and not intended to be manually entered. The inter-character delay is set to a small value, roughly 50 ms, so that slow typing of a custom command will be not recognized past the first character. A Trigger ON or Trigger OFF command greater than a single character must be sent as a string from another application.

Note: default,DMAE50,DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM080, DM280, DM470,DM580, DM503,DM7500