View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What can I set in the Inputs/Outputs step?

The behaviour of the buttons, input and output lines can be set in this pane. The details for a pulse encoder and the beeper pulse length can also be set here. This pane also has the link to the image buffer settings to FTP images to a server.

Note: default,DM050,DM060,DM070,DMAE50,DM150,DM260,DM300,DM360, DM370, DM080, DM280, DM470,DM580, DM503,DM7500,DM8050,DM8070,DM8600,DM8700,DM8700Base,DM8000Base,MX-1000,MX-1500