View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is the Interval Assistant?

The Interval Assistant, in Self and Continuous trigger modes, recommends a maximum interval time based on parameters you select.

First set the Application Type in the top left corner, and then click the Interval Assistant.

For In-Motion type applications, you have three options to calculate the necessary data. In the top right corner, select the units (standard or metric) you wish to calculate in.

- Select Field of View Size to calculate the longest possible interval time by measuring the physical field of view and giving the maximum line speed and the size of the longest code.
- Select Lens / Distance to Code if you want to give the distance of the code from the lens. Give the focal length and select the direction in which the code is travelling. Here you also need to give the maximum line speed and the size of the longest code.
- Select Code Element Size to calculate with the size of the most narrow code element. Enable Test Mode to read your code. You also need to give the direction your code is travelling in, the maximum line speed and the size of the longest code.

At the bottom of the Assistant you get the recommended maximum interval time.

For Hand Presentation type applications, present your code(s) to the reader in the various positions you will read them. The Assistant analyzes the decode time data and recommends a maximum interval time.

Note: DMAE50,DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM080, DM280, DM470,DM580, DM503