View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What can I set with the Used Communication Channel drop-down menu?

Here, you can set the communication method via USB. Depending on the used device, the following options are available:

- USB-COM only: Choose this option to reach the device through a serial port.

- USB-HID only: This option ensures that the device will behave like a USB keyboard.

- USB-COM + USB-HID: This is a combination of the above modes.

NOTE: In the case of USB-COM only, some devices may also be listed under 'HID devices', even though they lack HID functionality.
Note: DMAE50,DM050,DM060,DM070,DM8050,DM8070,DM8600,DM8700,DM8700Base,DM8000Base