View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What values can I set for the Height Sensor?

To calibrate the Package Height Sensor relative to your reader, first select one of the supported sensors you want to use: either the Omron Light Curtain RS232 or the Baumer Laser Ranger Finder RS232.

With the Omron Light Curtain, you can set the following values:

- Beam Spacing: distance in mm between beams, with a range of 0 – 300 mm
- Sensor to Surface: the distance between the conveyor and the package height sensor, with a range of 0 – 10,000 mm. On the height sensor, measure from the zero height point, using the calibration mark.

With the Baumer Laser Ranger Finder, you can set only the Sensor to Surface value.

Note: DM503