View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is the Image Buffer Maximum size?

Image Buffer Maximum Size is the maximum number of images that may be buffered on the reader. This is limited by the memory on the reader, but may be set to a number less than the maximum to prevent more than the desired number of images to be saved on the FTP server or PC.

Note that in Burst mode, the Burst Length + the Image Buffer Maximum Size must equal the maximum number of image buffers on the reader. The Setup Tool will automatically reduce the Image Buffer Maximum Size if the Burst Length is increased such that Burst Length + Image Buffer Maximum Size is larger than the maximum number of buffers on the reader.

Since the buffers to store images on the device and the buffers for image processing are shared, it is recommended to lower the number of stored images in Single Shot mode, too, in case a series of images is taken and the trigger rate is high. This will ensure that the device has enough buffers for normal processing.

Note: default,DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM080, DM280, DM470,DM580, DM503