# MX-1502 Specifications

Specification | MX-1100 Imager
--- | ---
Weight | 499g (664g with pistol grip)
Operating Temperature | 0ºC— +40ºC (+32ºF — +104ºF)
Storage Temperature | -10ºC — +60ºC (+10ºF — +140ºF)
Charging Temperature | 0ºC — +35ºC (+32ºF — +95ºF)
Maximum Humidity | < 95% (non-condensing)
Environmental | IP65
Codes | 1-D: UPC/EAN/JAN, Codabar, Interleaved 2 of 5, Code 39, Code 128, Code 93, Pharmacode, GS1 DataBar, PDF417, Micro PDF417 2-D: Data Matrix, QR Code, and MicroQR Code, DotCode and postal code
Power Supply Requirements | Battery power
Expected operating time for typical scan batches (400 scan per hour) with a fully charged battery | 12 hours

Note: The operating and charging temperature may be lower depending on the installed mobile phone.