# IMAGEBUFFER.TRANSFER-MODE

Sets or gets whether buffered images should automatically sent FTP or if they should be send only after requested.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
interval | enum | [0-1] | 0: On Request 1: FTP - runtime

## Platforms

DM60, DM70, DM80, DM280, DM300, DM360, DM370, DM470, DM8000, DM503, MX-1000, DM260.

## Notes

Version: 4.0.0