# CAMERA.MAX-EXPOSURE-US

Maximum exposure limit in microseconds for autoregulation.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
exposure | int | [1-50] | with HPIA
|  | [1-410] | without HPIA
|  | [1-100000] | with external or no illumination

## Platforms

DM70, DM80, DM150, DM260, DM280, DM300, DM360, DM370, DM470, DM503

## Notes

Version: 4.0.0