# LIGHT.DIRECT

Please note, that this command is deprecated. It is recommended to use LIGHT.BANKS command as an alternative with the same functionality. Sets the quadrants on the DM70, DM150 and DM260. Possible values are ON and OFF for each segment. Example for a SET command: SET LIGHT.DIRECT ON OFF OFF ON if you want to have the top-left and bottom-right LED on.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
north-east | bool | [ON|OFF] | enable/disable
north-west | bool | [ON|OFF] | enable/disable
south-east | bool | [ON|OFF] | enable/disable
south-west | bool | [ON|OFF] | enable/disable

## Platforms

DM70, DM150 and DM260 readers

## Notes

Version: 5.5.0