# CAMERA.AUTO-REGULATION

If enabled, the exposure time is adjusted after each acquisition to have optimal image brightness.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
auto |  | [ON|OFF] | ON: Automatic OFF: Manual

## Platforms

DM50, DM60, DM70, DM80, DM150, DM260, DM280, DM503, DM8600, and DM300, DM360, DM370, DM470

## Notes

Version: 5.6.0