# HPIT.INDICATOR-ON-TIME

Allows to control the Indicator0 (Green LED) on time to be executed in the following illumination pulse after an event has been detected.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
IND_ID | int | [0-1] | 0 = Left indicator 1 = Right indicator
TIME_US | int | [100-10000] |

## Platforms

DM370, DM470

## Notes

Version: 6.1.6