# SET-WIRELESS.LINK-TIMEOUT

Sets the keep alive timeout for wireless links. This command controls the balance between how quickly the reader detects the loss of wireless link and the ability to transfer large amount of data between the reader and base station. For detecting the loss of wireless link, a lower value means quicker detection. For transferring data, a higher value means better data transmission.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
Link timeout [s] |  | 0-65535 | Link timeout in seconds, 0 means infinite.

## Platforms

DM8700 Bluetooth reader

## Notes

Version: 6.2.7