# CONFIG-BACKUP.IP-ADDRESS

IP address of the Cognex Explorer FTP service.

Note: Uses dotted decimal form, such as "192.168.23.42".

## Actions

SET/GET PropertyCommand

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
string |  |  |

## Platforms

Ethernet readers. DM8000 wireless readers also support FTP if the base station is connected through Ethernet.

## Notes

Version: 5.0.0