# CQ.MINPASS

Code Quality Minimum Passing Grade. Determines the threshold for "validation failure action" including beep and configured line output.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
metric |  | [0-1] | 0: AIM-DPM/ISO/IEC TR 29158 1: ISO/IEC 15415
min-pass |  | [0-4] | 0: F 1: D 2: C 3: B 4: A

## Platforms

DM8600V

## Notes

Version: 3.0.0