# MIRROR.PATH

Sets/Gets the mirror positions string in execution for the reader. This command is designed to be used in sequential trigger modes not requiring the user to set the position manually. Note: Updating the path should be performed outside of the regular run time operation and angleA is limited to 0.0° without the Mirror2Axis feature key. If the same path is set multiple times in a row, the return of the path would be successful, but no extra operation will be executed.”

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
string | data | [0-512] | String syntax is "number_of_position_pairs:angle A0,angle B0;angle A1,angle B1;..." Example string is “2:10.5,10.5;10.5,10.5;”. Maximum of 64 positions, with value accuracy of 0.001° tolerance. Each value has a float format and therefore a round position needs to at least present one decimal point (eg 10 should be 10.0).

## Platforms

DM370, DM470 equipped with High Speed Steerable Mirror

## Notes

Version: 6.1.10