# PCM.METRIC-PARM-REPORT

Include the metric grading result for selected quality standard and metric in the report if enabled. Only available if not use for overall calculation (e.g. ISO-IEC 15415 → Modulation → Show in Report = ON) Not all metrics are available for each standard: AIM-DPM (0, 1, 2, 3, 4, 5, 6, 8), ISO-IEC 15415 (0, 1, 2, 3, 4, 5, 6, 7), ANSI-ISO-IEC 15416 (0, 4, 8, 9, 22, 23, 24, 25), SemiT10 (1, 4, 12, 13, 14, 15, 16, 17, 18, 19, 20), 1D readability (0, 2, 8, 9, 10, 11), DotCode (0, 1, 2, 3, 6, 8).

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
type |  | [0-5] | 0: AIM-DPM 1: ISO-IEC 15415 2: ANSI-ISO-IEC 15416 3: SemiT10 4: 1D readability 5: DotCode Readybility
type |  | [0-27] | 0: Symbol Contrast 1: Axial Non Uniformity 2: Print Growth 3: UEC 4: Modulation 5: Fixed Pattern Damage 6: Grid Non Uniformity 7: Extreme Reflectance 8: Reflect Min 9: Edge Contrast Min 10: Single Scan Int 11: Multi Scan Int 12: Signal To Noise Ratio 13: Horizontal Mark Growth 14: Vertical Mark Growth 15: Data Matrix Cell Width 16: Data Matrix Cell Height 17: Horizontal Mark Misplacement 18: Vertical Mark Misplacement 19: Cell Defects 20: Finder Pattern Defects 21: Overall Grade 22: Edge Determination 23: Defects 24: Reference Decode 25: Decodability 26: Contrast Uniformity 27: Reflectance Margin
state |  | [ON|OFF] | ON: include in report OFF: do not include in report

## Platforms

PCM-enabled readers

## Notes

Version: 5.7.0