# IMAGEBUFFER.NO-READ-IMAGE-RATE-COUNT

Number of bad read images to be buffered at a time unit (for example, minutes or hours) specified with IMAGEBUFFER.NO-READ-IMAGE-RATE-COUNT.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
interval | int |  |

## Platforms

DM80, DM280, DM503, DM300, only in Single, Burst, Self and Continuous modes.

## Notes

Version: 5.2.0