# ACCEL-SENSOR.OPERATION-MODE

Configures the application of the acceleration sensor.

Note: This command is only valid for Bluetooth-connected readers.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
int |  | [0-1] | 0: Acceleration Sensor is not used for waking the reader up from hibernation. 1: Acceleration Sensor is used for waking the reader up from hibernation.

## Platforms

DM8050, DM8600.

## Notes

Version: 5.4.0