# COM.DMCC-DEFAULT-TARGET

Determines whether the subsequent DMCC commands are executed on the Base Station or the Reader. The target you choose becomes the default setting, which persists after a device reboot.

## Actions

SET/GET Property

## Arguments

Name | Type | Range | Meaning
--- | --- | --- | ---
target | enum | [0,1] | 0: Base Station 1: Reader

## Platforms

DM8700 Base

## Notes

Version: 6.2.5