View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# Will further images be taken once a valid reading occurs?

No. Once a setup produces a valid image, the reader will no longer try additional setups during that trigger cycle. It will start decoding when it finds a valid image. Additional images are taken when readings in previous setups fail. The reader will try each enabled setup in a priority order, starting at the specified highest priority setup, and move on until a valid reading is taken.

Note: DM070,DM150,DM260,DM300,DM360, DM370, DM080, DM280, DM470,DM580, DM380, DM503,DM8600,DM8700,MX-1000,MX-1500