View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What is the What Results to Buffer list for?

The What Results to Buffer list allows you to choose which type of images are internally buffered on the reader, whether they contain decode information (Read), no decode information (NoRead), both (All) or Validation Failure, in which case only images of successful decoding, but validation failure will be stored.

However, be aware that in Burst and Continuous Modes all images of the whole sequence are stored based on the decision whether the sequence was Read or NoRead. For Burst mode, the whole sequence means all acquired images specified by the burst count. In Continuous mode, triggering acquires images as long as the trigger signal remains active, which means that all images are stored and saved until the trigger signal ends.

Note: default,DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM080, DM280, DM470,DM580, DM380, DM503