View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What other options are there on the Verification tab?

At present, AIM-DPM/ISO/IEC TR29158 is supported for verification. You can set the Minimum Pass Grade in the Quality Metrics area on the tab. This setting is the minimum grade that the verification gives a Pass to when grading symbol metrics. If ticked, Graphics Enabled allows scalable vector graphics to appear on problematic areas of the read code in the Image Pane.

See more information on other setting below.

Note: DM8600