View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# What are the individual options in the General tab in the Data field of the Standard tab?

- Sub-string: A sub-string of the characters encoded in the symbol. You must specify a range for the sub-string to use this option.

- Full string: All of the characters encoded in the symbol

- Decode time: The amount of time, in milliseconds, it took the reader to decode the symbol. This period of time does not include image acquisition, pending image processing, communication time and additional processing (for example, Data Formatting).

- Trigger time: The amount of time, in milliseconds, between when the trigger was received and when the decode operation was complete

- Symbology: The symbology of the decoded symbol

- CR/LF: Carriage Return with Line Feed

- TAB: A tab character.

- SP: A space character.

- Symbology Identifier: The symbology identifier as specified by ISO/IEC 15424:2008

- Module Size: The width (or height), in pixels, of each module in the symbol

- Code Position: The image coordinates of each corner of the decoded symbol

- Code Orientation: The orientation of the decoded symbol reported in degrees. Clockwise rotations of the decoded symbol are considered positive changes in orientation.

- Contrast: A value, between 0 and 1, to indicate the total amount of contrast within the decoded symbol. A high value indicates the light and dark modules in the symbol have a wide range of grey values, while a low value indicates the light and dark modules consist of similar grey values.

- UEC: The amount of available unused error correction in the symbol. Error correction is a method of reconstructing or replacing data that is lost through symbol damage. A value of "100" is ideal. 1D Symbology always returns -1.

- Input string: The received (serial or Ethernet) input string.

- Filter time: The duration of filtering in milliseconds (ms).

- Result source: The name of the device.

All of following values will increment whether or not the reader is connected to the Setup Tool.

- Total Reads: The total number of decoded symbols

- Total NoReads: The number of times a trigger was received but no symbol was decoded

- Total Triggers: Total Triggers = Total Reads + Total NoReads + Total Missed Triggers

- Missed Triggers: The number of missed triggers because no image buffer was available when the trigger was detected

- Trigger Index: The total number of triggers detected by the reader.

Values that will be reset to 0 any time when either the Process Statistics is cleared on the Process Monitor pane, or after a reader reboot are the following:

- Total Reads

- Total NoReads

- Total Triggers

- Missed Triggers

Trigger Index will be reset to 0 only after a reader reboot, but not after clearing the Process Statistics.

Note: default,DMAE50,DM050,DM060,DM070,DM150,DM260,DM300,DM360, DM370, DM080, DM280, DM470,DM580, DM380, DM503,DM7500,DM8050,DM8070,DM8600,DM8700,MX-1000,MX-1500