View: All

Select your DataMan Reader:

All

DataMan 50

DataMan 60

DataMan 70

DataMan 80

DataMan 150

DataMan 260

DataMan 280

DataMan 300

DataMan 360

DataMan 370

DataMan 380

DataMan 470

DataMan 503

DataMan 580

DataMan 7500

DataMan 8050

DataMan 8070

DataMan 8600

DataMan 8700

DataMan 8700 Base Station

Base Station

DataMan MX-1000

DataMan MX-1500

# I still cannot connect to my reader: Can I reset it?

Print a copy of the Configuration Codes document for your particular reader, available through the Windows Start menu or the Setup Tool Help menu.

Scan the Reboot Scanner code to perform a soft reset. The reader's nonvolatile memory is not cleared, but the reader is shut down and restarted.

If you still cannot connect to the reader, scan the Reset Scanner to Factory Defaults code to return the reader to its factory-default state.

If that fails to clear the issue, disconnect the reader from power (both DC power and USB, if connected). While holding down the trigger button, reconnect the reader to power. Keep pressing the trigger button for at least 6 seconds, until the double beep occurs. The reader will flash its indicator lights in different colors.

Note: DMAE50,DM050,DM060,DM070,DM150,DM260,DM300,DM360,DM370, DM080, DM280,DM470,DM580, DM380,MX-1000,MX-1500